A screenshot of a computer

Description automatically generated

**Figure S1. Graphical representation of pipette tip wetting procedure.** (**A**) Aspirate the sample or stock solution and add it back to the tube by pressing down on the plunger to the first stop (blue box). (**B**) If residual liquid remains in the pipette tip (red box), aspirate the desired volume and repeat the process. (**C**) Look for a consistent volume of residual liquid left in the pipette tip at the first stop (yellow box). (**D**) Lastly, aspirate the desired volume and add/transfer to sample tubes in identical fashion (purple box). Graphic was prepared in BioRender.